============================================================================

KONICA MINOLTA bizhub 350/250/200 Printer
Printer Software Document

============================================================================
This document contains information about the software of
KONICA MINOLTA bizhub 350/250/200.
In addition, the problem that may happen when the software of this version is 
used, and the solutions are mentioned.
Read through this document before you use KONICA MINOLTA bizhub 350/250/200.

****************************************************************************

Readme File Contents

****************************************************************************
1. Printer Driver Installer
2. Attentions and Restrictions

///////////////////////////////////////////////////////////////////////////////
1. Printer Driver Installer
///////////////////////////////////////////////////////////////////////////////

This document describes following information about the Printer Driver 
Installer.

1.Version Information
2.Attention
3.File Composition
4.Installing the Software
5.How to check the Version

1.Version Information
  This document explains the following installer version.

  KONICA MINOLTA Printer Driver Installer Ver.5.1.1.1
  (For Windows NT 4,Windows 2000/XP/Server 2003)

2.Attention
  Please read the following notes before use.
2-1.The following operating environment is required in order to start the 
    Installer on Windows NT 4.0.
  - The newest service pack SP6a needs to be installed.
  - The Internet Explorer needs to be updated by 4.0 or more.
  - In order to start the Help File by pressing the Help bottom on the 
    Installer, HTML Help Runtime Component Ver1.3 or more is necessary to be 
    installed in the computer beforehand. (In NT4, this program may not be 
    installed as standard depending on the OS language. In that case, please 
    download the HTML Help Runtime Component Ver1.3 or more from Microsoft site
    and install it.)
2-2.When you start the installer by Windows NT 4.0/2000/XP/Server 2003 and 
    install the printer, it is necessary to log in by the user who has the
    administrator power to the installing computer. Power User cannot 
    install it.
2-3.It is possible to set the installed printer to be used from other computer
    on Windows NT 4.0/2000/XP/Server 2003. 

3. File Composition
  [Driver] Folder
    |-[Driver] Folder
        |-[PCL]
            |- [DE]               PCL Driver for German
            |- [EN]               PCL Driver for English
            |- [ES]               PCL Driver for Spanish
            |- [FR]               PCL Driver for French
            |- [IT]               PCL Driver for Italian
            |- [JA]               PCL Driver for Japanese
            |- [KO]               PCL Driver for Korean
            |- [ZH-CN]            PCL Driver for Simplified Chinese
            |- [ZH-TW]            PCL Driver for Traditional Chinese
    |-[Lang] Folder               Various Setting for each language/Help files
    |-[Bmp] Folder                Bitmap file used in installer
    |-[Readme] Folder
        |-[EN]
            |- [Readme.txt]       Readme file for English (This file)
        |-[JA]
            |- [Readme.txt]       Readme file for Japanese
    |-[setupsub] Folder           Subdirectory for this installer
    |-[Setup64.exe]               Printer Driver Installer
    |-[Setup.exe]                 Printer Driver Installer

4.Installing the Software
  Double click the Setup.exe file and perform the installation according to
  the Wizard of screen.
  However, when you print using Parallel Port or USB Port, please install the  
  Printer Driver by using the Plug&Play function of the Operating System.
  
5.How to check the Version
  Please check the version information from the property of Setup.exe icon.


///////////////////////////////////////////////////////////////////////////////
2. Attentions and Restrictions
///////////////////////////////////////////////////////////////////////////////

KONICA MINOLTA bizhub 350/250/200 offers many convenient functions.
Depending on the application, similar functions are realized by itself.
In such a case, please be careful of the setting method etc.

Attentions and Restrictions of each functional detail are shown below.

(1)Paper Size Setting
  1)When not printing as paper size setting
    - Paper size can be specified by Printer property,
      but it may become invalid the paper size that is set on the printer 
      property according to an application.
      ==>Please set the paper size on [Print...] menu of an application.
      
(2)Paper Source Setting
  1)Cannot set Paper Source
    - To set Tray3, Tray4 or LCT for Paper Source, the optional Paper Sources is
      necessary. Also, you need to set the Tray at the option of the printer.
      ==>Please check the existence of Paper Source and the setting
         of the printer option.
    - Paper Source may have restriction depending on the specified paper size.
  2)When paper source method doesn't work as specified.
    - Paper source can be set by Printer property, 
      but it may become invalid the paper source that is specified on the
      printer property according to an application.
      ==> Please set the paper source on [Print...] menu of an application.
    - Paper may be fed from a different tray other than the tray specified
      depending on the paper size set up on the machine.

(3)Print Orientation Setting
  1)Print orientation setting doesn't work as specified.
    - Print Operation can be set by Printer property, 
      but it may become invalid the Print Orientation that is specified on the 
      printer property depending on an application.
      ==> Please set Print Orientation on [Page Setup...] menu in an application
(4)Collate Functions
  1)Collate doesn't work as specified.
    Collate is able to be set by Printer property, but the following situation
    may occur depending on an application if you specify Collate on 
    [Print...] menu.
    - If "Combination" function is specified, the last page of No. n copies and
      the first page of No. n+1 copies are printed on the same paper.
    - If "Double-Sided" function is specified, the first page of No. n+1 copies
      is printed on the reverse side of the last page of No. n copies.
    - If "Booklet" function is specified, all prints are collected into one book
      and printed.
    - If "Staple" function is specified, all prints are collected into one set 
      and stapled.
    - If "Distribution Number Stamping" function is specified, all prints are
      printed with the same Number Stamp.
    - If "Secure print" function is specified, the waiting documents for
      print for specified number of copies are stored in the machine.
    - If "Watermark" function is specified only on the first page of
      multiple copies of printing, it will be stamped only on the first page of
      the first copy.
    - Even if "Offset" function is specified, it will be output without offset.
    - If "Proof and Print" function is specified, all prints are printed 
      without storing.
    - If "Cover Page" function is specified, cover page is not inserted in 
      the right place. 
    - If "Per Page Setting" function is specified, it doesn't operate with 
      correct page number.
    ==>Please set No Collate on [Print...] menu and specify Collate on the 
       Printer property.

(5)Copies Setting
  1)Copies Setting doesn't work as specified.
    Copies can be set by Printer property and Print menu of the most of an
    application, but the priority of setting between Printer property setting
    and [Print...] menu setting is different depending on an application.
    ==>First, please set 1 for the copies on [Print...] menu and specify the 
       required copies by the Printer property.
       If only 1 copy is printed with this setting, please specify the required
       copies on [Print...] menu.
  2)Proof and Print, and Copies
    In Excel, even though Proof and Print function is selected and multiple 
    copies are set for print, all copies of document will be printed without
    storing.
    *Proof and Print function cannot be specified with 1 copy. Also, even if 
     the multiple copies are set in Excel-copy unit print/ON, Proof and Print
     function is cancelled because all data are printed only 1 copy with number
     of set.
     This can be solved by un-checking [Print on copy unit].

(6)Front Cover Page/Back Cover Page
  1)Paper for Front/Back Cover Page
     When you use Front Cover Page Function and Back Cover Page Function, it is
     necessary to set the correct paper beforehand in the Paper Source for 
     Front Cover Page/Back Cover Page that is specified by the printer driver.

(7)User Authentication/Account Track
  1)Printing under User Authentication and Account Track
    When you use the printer that requires User Authentication/Account Track 
    before printing, print is not accepted without entering the correct User 
    Name, Department Name and Password.   

(8)When you print by using LPR protocol from Windows XP 
  1)Please check "LPR Byte Counting Enabled".
    Depending on the state of the communication, it cannot be printed.

(9)Others
  1)When sending plural printing job to Local Port/Network Port
     If multiple copies of document is sent to each port such as Parallel, IPP,
     SMB, RAW and LPR at the same time. The print out of one set of document 
     may be separated by another print job. 
     ==> In this case, select Uncollated.
  2)When the upper limit value is exceeded at the Account Track
     When "Copy Track Mode" and "Copy Limit" are set to "Yes", if there is a 
     job that stops in the middle of printing as the limit is reached, the 
     later print jobs are not output unless the stopping job is canceled.
     ==>The administrator must cancel the "Copy Limit" to output the stopping 
        job or someone must delete the job after confirmation. 
  3) Power OFF while printing/processing
    Do not turn off the machine while it is printing/processing as a 
    malfunction may occur. If the power is turned off by mistake, and 
    a malfunction occurs, turn off the machine once and then turn it on again.
  4)Copies Setting in Application
    Depending on an application, you can enter exceeding 999 for copies, but
    only one copy may be printed.
  5)Registration of Custom Size
    Please perform registration of Custom Size in WindowsNT4/2000/XP 
    by administrator. 
  6)If you perform Staple or Punch to the mixed originals with different 
    paper size and image orientation, it may not be stapled or punched on the 
    specified place.
  7)After double-sided printing of the originals with mixed paper size 
    if you change into single-sided print setting by the printer operation
    panel, white paper may be inserted at the place where the paper size 
    is changed.

============================================================================

Microsoft, Windows, and Windows NT are the registered trademarks for the 
United States and other countries of US Microsoft companies.
Additionally, company names and product names written in this document are the
registered trademarks or trademarks of their respective companies.

(C)2005-2009 KONICA MINOLTA BUSINESS TECHNOLOGIES, INC.
============================================================================