============================================================================

KONICA MINOLTA bizhub 350/250/200 Printer
Printer Software Document

============================================================================
This document contains information about the software of
KONICA MINOLTA bizhub 350/250/200.
In addition, the problem that may happen when the software of this version is 
used, and the solutions are mentioned.
Read through this document before you use KONICA MINOLTA bizhub 350/250/200.

****************************************************************************

Readme File Contents

****************************************************************************
1. Printer Driver Installer
2. Attentions and Restrictions

///////////////////////////////////////////////////////////////////////////////
1. Printer Driver Installer
///////////////////////////////////////////////////////////////////////////////

This document describes following information about the Printer Driver 
Installer.

1.Version Information
2.Attention
3.File Composition
4.Installing the Software
5.How to check the Version

1.Version Information
  This document explains the following installer version.

  KONICA MINOLTA Printer Driver Installer Ver.5.1.1.1
  (For Windows 2000/XP/Server 2003)

2.Attention
  Please read the following notes before use.
2-1.When you start the installer by Windows 2000/XP/Server 2003 and 
    install the printer, it is necessary to log in by the user who has the 
    administrator power to the installing computer. 
    Power User cannot install it.
2-2.It is possible to set the installed printer to be used from other computer
    on Windows 2000/XP/Server 2003. 

3. File Composition
  [Driver] Folder                 Driver for Windows 2000/XP/Server 2003
    |-[Driver] Folder
        |-[PS]
            |- [DE]               PS Driver for Germany
            |- [EN]               PS Driver for English
            |- [ES]               PS Driver for Spanish
            |- [FR]               PS Driver for French
            |- [IT]               PS Driver for Italy
            |- [JA]               PS Driver for Japanese
            |- [KO]               PS Driver for Korean
            |- [ZH-CN]            PS Driver for Simplified Chinese
            |- [ZH-TW]            PS Driver for Traditional Chinese
    |-[Lang] Folder               Various Setting for each language/Help files
    |-[Bmp] Folder                Bitmap file used in installer
    |-[PPD-PageMaker] Folder
        |- [English]              PageMaker Driver for English
        |- [French]               PageMaker Driver for French
        |- [German]               PageMaker Driver for Germany
        |- [Italian]              PageMaker Driver for Italy
        |- [Japanese]             PageMaker Driver for Japanese
        |- [Korean]               PageMaker Driver for Korean
        |- [Simplified Chinese]   PageMaker Driver for Simplified Chinese
        |- [Spanish]              PageMaker Driver for Spanish
        |- [Traditional Chinese]  PageMaker Driver for Traditional Chinese
    |-[Readme] Folder
        |-[EN]
            |- [Readme.txt]       Readme file for English (This file)
        |-[JA]
            |- [Readme.txt]       Readme file for Japanese
    |-[setupsub] Folder           Subdirectory for this installer
    |-[Setup64.exe]               Printer Driver Installer
    |-[Setup.exe]                 Printer Driver Installer

4.Installing the Software
  Double click the Setup.exe file and perform the installation according 
  to the Wizard of screen

5.How to check the Version
  Please check the version information from the property of Setup.exe icon.



///////////////////////////////////////////////////////////////////////////////
2. Attentions and Restrictions
///////////////////////////////////////////////////////////////////////////////

KONICA MINOLTA bizhub 350/250/200 offers many convenient functions.
Depending on the application, similar functions are realized by itself.
In such a case, please be careful of the setting method etc.

Attentions and Restrictions of each functional detail are shown below.

(1)Paper Size Setting
  1)When not printing as paper size setting
    - Paper size can be set by the Printer property, 
      but it may become invalid the paper size that is specified on the 
      printer property according to an application.
      ==>Please set the paper size on [Print...] menu of an application.

(2)Paper Source Setting
  1)Cannot set Paper Source
    - To set Tray3, Tray4 or LCT for the Paper Source, the optional Paper 
      Sources is necessary. Also, you need to set the Tray at the option of the
      printer.
      ==> Please check the existence of Paper Source and the setting of the 
          printer option.
    - Paper Source may have restriction depending on the specified paper size.
  2)When paper source method doesn't work as specified
    - Paper source can be set by Printer property,
      but it may become invalid the paper source that is specified on the 
      printer property according to an application.
      ==> Please set the paper source on [Print...] menu of an application.
    - Paper may be fed from a different tray other than the tray specified 
      depending on the paper size set up on the machine.

(3)Print Orientation Setting
  1)Print orientation setting doesn't work as specified
    - Print orientation can be set by the Printer property,
      but it may become invalid the Print Orientation that is specified on the 
      printer property depending on an application.
      ==>Please set Print Orientation on [Page Setup...] menu in an application.      
(4)Collate Functions
  1)Collate doesn't work as specified.
    Collate is able to be set by Printer property, but the following situation
    may occur depending on an application if you specify Collate on [Print...] 
    menu.
    - If "Combination" function is specified, the last page of No. n copies and
      the first page of No. n+1 copies are printed on the same paper.
    - If "Double-Sides" function is specified, the first page of No. n+1 copies
      is printed on the reverse side of the last page of No. n copies.
    - If "Booklet" function is specified, all prints are collected into one book
      and printed.
    - If "Staple" function is specified, all prints are collected into one set
      and stapled.
    - If "Secure print" function is specified, the waiting documents for print
      for specified number of copies are stored in the machine.
    - If "Watermark" function is specified only on the first page of
      multiple copies of printing, it will be stamped only on the first page of
      the first copy.
    - Even if "Offset" function is specified, it will be output without offset.
    - If "Proof and Print" function is specified, all prints are printed 
      without storing.
    - If "Cover Page" function is specified, cover page is not inserted in 
      the right place.
    ==>Please set No Collate on [Print...] menu and specify Collate on the 
       Printer property.

(5)Copies Setting
  1)Copies Setting doesn't work as specified.
    Copies can be set by the Printer property and Print menu of the most of 
    an application, but the priority of setting between Printer property 
    setting and [Print...] menu setting is different 
    depending on an application.
    ==>First, please set 1 for the copies on [Print...] menu and specify the
       required copies by the Printer property.
       If only 1 copy is printed with this setting, please specify the required
       copies on [Print...] menu.
  2)Proof and Print, and Copies
    In Excel, even though Proof and Print function is selected and multiple 
    copies are set for print, all copies of document will be printed without 
    storing.
    * Proof and Print function cannot be specified with 1 copy. Also, even if 
      the multiple copies are set in Excel-copy unit print/ON, Proof and Print 
      function is cancelled because all data are printed only 1 copy with 
      number of set.
      This can be solved by un-checking [Print on copy unit].

(6)Front Cover Page/Back Cover Page
  1)Paper for Front/Back Cover Page
    When you use Front Cover Page Function and Back Cover Page Function, it is
    necessary to set the correct paper beforehand in the Paper Source for Front
    Cover Page/Back Cover Page that is specified by the printer driver.

(7)User Authentication/Account Track
  1)Printing under User Authentication and Account Track
    When you use the printer that requires User Authentication/Account Track 
    before printing, print is not accepted without entering the correct User 
    Name, Department Name and Password.
    
(8)When you print by using LPR protocol from Windows XP 
  1)Please check "LPR Byte Counting Enabled".
    Depending on the state of the communication, it cannot be printed.

(9)Others
  1)When sending plural printing job to Local Port/Network Port
    If multiple copies of document is sent to each port such as Parallel, IPP,
    SMB, RAW and LPR at the same time. The print out of one set of document 
    may be separated by another print job. 
    ==> In this case, select Uncollated.
  2)When the upper limit value is exceeded at the Account Track
    When "Copy Track Mode" and "Copy Limit" are set to "Yes", if there is a job
    that stops in the middle of printing as the limit is reached, the later 
    print jobs are not output unless the stopping job is canceled.    
    ==>The administrator must cancel the "Copy Limit" to output the stopping 
       job or someone must delete the job after confirmation.
  3)Power OFF while printing/processing
    Do not turn off the machine while it is printing/processing as a 
    malfunction may occur. If the power is turned off by mistake, and 
    a malfunction occurs, turn off the machine once and then turn it on again.
  4)Copies Setting in Application
    Depending on an application, you can enter exceeding 999 for copies, 
    but only one copy may be printed.
  5)When you print the multiple copies on the Microsoft Word while the several
    applications are running, in rare case only 1 copy is printed depending on 
    the specification of the OS or an application. In that case, close unused 
    applications and please try to print.
  6)If you perform Staple or Punch to the mixed originals with different 
    paper size and image orientation, it may not be stapled or punched on the 
    specified place.
  7)After double-sided printing of the originals with mixed paper size 
    if you change into single-sided print setting by the printer operation
    panel, white paper may be inserted at the place where the paper size 
    is changed.
  8)When you set the copies other than one for the printer default setting,
    the copies setting of the printer driver might not be operate correctly.
    In that case, please set the copies of default to one.
  9)You can not add printers as IPP printer on iPrint client of Novell Netware Ver.5 or later.
    It will fail to download the PS driver from your Netware Server when you try to add 
    printers.
    ==> When you need to add printers on the environment described above, please use PCL
    driver.


  -----------------------------------------------------
  Cautions and restrictions with specified applications
  -----------------------------------------------------
(1)Microsoft Office
  1)When you have your PC connect with the printer by SMB under Windows XP and try to
    print any documents written by Word2002 with Nin1 and Watermark function, Nin1
    function will not work correctly nor Watermark will be printed in a small font.
     ==> In this case, please print by any communication ports other than SMB.


============================================================================

Microsoft, and Windows are the registered trademarks for the United States and 
other countries of US Microsoft companies.
Additionally, company names and product names written in this document are the
registered trademarks or trademarks of their respective companies.

(C)2005-2009 KONICA MINOLTA BUSINESS TECHNOLOGIES, INC.
============================================================================